FirmwareUpdate.efi is used to update image on Intel(R) Desktop Board DQ57TM.

Intel(R) UDK2010 Firmware Update Utility for the Intel(R) Desktop Board DQ57TM
Version 0.95
Copyright(c) Intel Corporation 2006 - 2012

Usage: FirmwareUpdate [OPTIONS] [UPDATEFILE]
[OPTIONS]
  -f            Program entire flash device.
  -m MAC        Programs the MAC address for the on-board LAN device.  If the
                UPDATEFILE parameter is not provided only the MAC address will
                be updated.  The expected MAC address format is 0011AA33CC55
  -v            Includes the variable region (NVRAM) in the update.               

Example:
  FirmwareUpdate –f UDK_TM_B9_release.rom –m 0011AA33CC55

Notes:
   Before using FirmwareUpdate.efi to update ROM file, shutdown the system and
   put the motherboard in configuration mode (BIOS CFG Jumper, set pin 2-3).
   Please shutdown the system after the flash updates successfully and restore
   the system to normal operating mode (BIOS CFG Jumper, set pin 1-2).

Updates in Version 0.95:
   Fixed issue where some flash regions may be missed when performing a full SPI
   update.