


TFTP Upgrade Instructions

Before initiating the TFTP upgrade, please take a look at the following grid and make sure the right images are being used.  Also verify the file sizes are accurate, for the downloaded images.

======================================================================

Platform

Upgrading from

Image Files

Instructions

======================================================================

1.    
CACHEdirector
1.0.7/1.0.8


109_mp.180C

Step 1

======================================================================

======================================================================

TFTP Image

Size (in bytes)

Checksum (using cksum)

======================================================================

1.    
109_mp.180C


450968


2949327204

======================================================================

Step 1
Following are switch CLI commands/output:

/boot/tftp

Enter name of switch software image to be replaced

  ["image1"|"image2"|"boot"]: <choose image1 or image2>

Enter hostname or IP address of TFTP server: <enter local TFTP server IP address>

Enter name of file on TFTP server: 109_mp.180C

  (verify the number of bytes transferred with the original file size)

/boot/image <use the same image chosen above, to boot from>

/boot/reset


Check Images

Verify that the switch is running version 1.0.9 code by typing:

/info/sys 

