-- $Id: atmfima.mib,v 1.3 2000/07/12 15:19:20 ama Exp $
--
-- Feb 23, 2000: Initial release is based on SNMPv2 MIB.
--
-- Feb 29, 2000: Modified v2 based syntax to v1 based syntax
-- The following are the changes made:
--	* MODULE-IDENTITY, TEXTUAL-CONVENTION, NOTIFICATION-TYPE 
--	  are removed
--	* DateAndTime has been changed to TimeTicks
--	* MAX-ACCESS has been changed to ACCESS
--	* STATUS current has been changed to mandatory
--	* ACCESS read-create has been changed to read-write
--	* ACCESS accessible-for-notify has been changed to read-only
--	* ACCESS of imaGroupIndex, imaLinkIfIndex, imaGroupIntervalNumber
--	  imaLinkIntervalNumber have been changed from not-accessible to 
--        read-only 
--	* ACCESS of imaGroupRowStatus and imaLinkRowStatus have been
--	  changed to read-only
--	* InterfaceIndex has been changed to InterfaceIndex
--      * imaAlarmStatus & imaAlarmType are not supported
--
IMA-MIB DEFINITIONS ::= BEGIN

IMPORTS
--      MODULE-IDENTITY, OBJECT-TYPE, Integer32, Counter32, Gauge32,
--      NOTIFICATION-TYPE, enterprises
--        FROM SNMPv2-SMI
--      MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
--        FROM SNMPv2-CONF
--      TEXTUAL-CONVENTION, DateAndTime, RowStatus
--        FROM SNMPv2-TC
--      InterfaceIndex, InterfaceIndex, ifIndex

      InterfaceIndex, ifIndex
        FROM IF-MIB

      enterprises, IpAddress, TimeTicks
	FROM RFC1155-SMI

      atmForum, atmForumNetworkManagement
	FROM ATM-FORUM-TC-MIB

      OBJECT-TYPE
	FROM RFC-1212

      TRAP-TYPE
	FROM RFC-1215

      Counter32, Integer32, TimeStamp, RowStatus, TruthValue,
      Gauge32
	FROM SNMPv2-SMI-v1

      mib-2, DisplayString
	FROM RFC1213-MIB;

--  atmfImaMib MODULE-IDENTITY
--      LAST-UPDATED "9902111830Z"
--      ORGANIZATION "The ATM Forum"
--      CONTACT-INFO
--        "ATM Forum
--        World Headquarters
--        2570 West El Camino Real
--        Suite 304
--        Mountain View, CA 94040-1313
--        USA
--        Phone: +1 415 949 6700
--        Fax: +1 415 949 6705
--        email: info@atmforum.com"
--      DESCRIPTION
--        "The MIB module for managing ATM Forum Inverse Multiplexing
--        for ATM (IMA) interfaces."
--      REVISION     "9902111830Z"
--      DESCRIPTION
--        "Updated and repaired version of the IMA-MIB released with the
--        IMA v1.1 specification (af-phy-0086.001)."
--      REVISION     "9701092245Z"
--      DESCRIPTION
--        "Initial incomplete version of the IMA-MIB as published in the
--        IMA v1.0 specification (af-phy-0086.000)."
--      ::= { atmfIma 1 }

-- The object identifier subtree for the IMA-MIB.

atmfIma OBJECT IDENTIFIER ::= { atmForumNetworkManagement 7 }

atmfImaMib OBJECT IDENTIFIER ::= { atmfIma 1 }

atmfImaMibObjects OBJECT IDENTIFIER ::= { atmfImaMib 1 }
atmfImaMibTraps OBJECT IDENTIFIER ::= { atmfImaMib 2 }
atmfImaMibTrapPrefix OBJECT IDENTIFIER ::= { atmfImaMibTraps 0 }
atmfImaMibConformance OBJECT IDENTIFIER ::= { atmfImaMib 3 }

-- Textual conventions

--  MilliSeconds ::= TEXTUAL-CONVENTION
--    STATUS      current
--    DESCRIPTION
--        "Time in milliseconds"
--    SYNTAX      Integer32
    MilliSeconds ::= Integer32

--  ImaGroupState ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "State of the IMA group."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 10.2.1 on page 55"
--      SYNTAX      INTEGER {
--        notConfigured(1),
--        startUp(2),
--        startUpAck(3),
--        configAbortUnsupportedM(4),
--        configAbortIncompatibleSymmetry(5),
--        configAbortOther(6),
--        insufficientLinks(7),
--        blocked(8),
--        operational(9),
--        configAbortUnsupportedImaVersion(10) }
    ImaGroupState ::= INTEGER {
        notConfigured(1),
        startUp(2),
        startUpAck(3),
        configAbortUnsupportedM(4),
        configAbortIncompatibleSymmetry(5),
        configAbortOther(6),
        insufficientLinks(7),
        blocked(8),
        operational(9),
        configAbortUnsupportedImaVersion(10) }

--  ImaGroupFailureStatus ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "Failure reason of an IMA group."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 10.2.1, page 55"
--      SYNTAX      INTEGER {
--        noFailure(1), -- unit is up
--        startUpNe(2),
--        startUpFe(3),
--        invalidMValueNe(4),
--        invalidMValueFe(5),
--        failedAssymetricNe(6),
--        failedAssymetricFe(7),
--        insufficientLinksNe(8),
--        insufficientLinksFe(9),
--        blockedNe(10),
--        blockedFe(11),
--        otherFailure(12),
--        invalidImaVersionNe(13),
--        invalidImaVersionFe(14) }
    ImaGroupFailureStatus ::= INTEGER {
        noFailure(1), -- unit is up
        startUpNe(2),
        startUpFe(3),
        invalidMValueNe(4),
        invalidMValueFe(5),
        failedAssymetricNe(6),
        failedAssymetricFe(7),
        insufficientLinksNe(8),
        insufficientLinksFe(9),
        blockedNe(10),
        blockedFe(11),
        otherFailure(12),
        invalidImaVersionNe(13),
        invalidImaVersionFe(14) }

--  ImaAlarmStatus ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "A qualification of the IMA trap which indicates if the
--        condition causing the trap has been detected (declared)
--        or is no longer present (cleared)."
--      SYNTAX      INTEGER {
--        cleared(1),
--        declared(2) }
    ImaAlarmStatus ::= INTEGER {
	cleared(1),
	declared(2) }

--  ImaAlarmType ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "An identification of the event that caused the generation
--        of the IMA trap."
--      REFERENCE
--       "ATM Forum IMA v1.1, Section 12.2.3 on page 79"
--      SYNTAX      INTEGER {
--        imaAlarmLinkLif(1),
--        imaAlarmLinkLods(2),
--        imaAlarmLinkRfi(3),
--        imaAlarmLinkTxMisConnect(4),
--        imaAlarmLinkRxMisConnect(5),
--        imaAlarmLinkTxFault(6),
--        imaAlarmLinkRxFault(7),
--        imaAlarmLinkTxUnusableFe(8),
--        imaAlarmLinkRxUnusableFe(9),
--        imaAlarmGroupStartupFe(10),
--        imaAlarmGroupCfgAbort(11),
--        imaAlarmGroupCfgAbortFe(12),
--        imaAlarmGroupInsuffLinks(13),
--        imaAlarmGroupInsuffLinksFe(14),
--        imaAlarmGroupBlockedFe(15),
--        imaAlarmGroupTimingSynch(16) }
    ImaAlarmType ::= INTEGER {      
        imaAlarmLinkLif(1),
        imaAlarmLinkLods(2),
        imaAlarmLinkRfi(3),
        imaAlarmLinkTxMisConnect(4),
        imaAlarmLinkRxMisConnect(5),
        imaAlarmLinkTxFault(6),
        imaAlarmLinkRxFault(7),
        imaAlarmLinkTxUnusableFe(8),
        imaAlarmLinkRxUnusableFe(9),
        imaAlarmGroupStartupFe(10),
        imaAlarmGroupCfgAbort(11),
        imaAlarmGroupCfgAbortFe(12),
        imaAlarmGroupInsuffLinks(13),
        imaAlarmGroupInsuffLinksFe(14),
        imaAlarmGroupBlockedFe(15),
        imaAlarmGroupTimingSynch(16) }

--  ImaGroupTxClkMode  ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "Indicate the transmit clock mode of the IMA group.
--        There are two possible modes: the Common Transmit
--        Clock (CTC) and the Independent Transmit Clock (ITC).
--        The CTC mode corresponds to the case when the transmit clock
--        of all IMA links are derived from the same source.  The ITC
--        configuration corresponds to the case where there is at least
--        one IMA link whose transmit clock is derived from a source
--        different than at least another link transmit clock."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 7 on page 38"
--      SYNTAX      INTEGER {
--        ctc(1),
--        itc(2) }
    ImaGroupTxClkMode  ::= INTEGER {
	ctc(1),
	itc(2) }

--  ImaGroupSymmetry ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "The group symmetry mode adjusted during the group start-up."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 5.2.2.7 on page 35"
--      SYNTAX      INTEGER {
--        symmetricOperation(1),
--        asymmetricOperation(2),
--        asymmetricConfiguration(3) }
    ImaGroupSymmetry ::= INTEGER {
	symmetricOperation(1),
	asymmetricOperation(2),
	asymmetricConfiguration(3) }

--  ImaFrameLength ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "Length of the IMA frames."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 5.2.2.4.2 on page 34"
--      SYNTAX      INTEGER {
--        m32(32),
--        m64(64),
--        m128(128),
--        m256(256) }
    ImaFrameLength ::= INTEGER {
	m32(32),
	m64(64),
	m128(128),
	m256(256) }

--  ImaLinkState ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "State of a link belonging to an IMA group."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
--      SYNTAX      INTEGER {
--        notInGroup(1),
--        unusableNoGivenReason(2),
--        unusableFault(3),
--        unusableMisconnected(4),
--        unusableInhibited(5),
--        unusableFailed(6),
--        usable(7),
--        active(8) }
    ImaLinkState ::= INTEGER {
	notInGroup(1),
	unusableNoGivenReason(2),
	unusableFault(3),
	unusableMisconnected(4),
	unusableInhibited(5),
	unusableFailed(6),
	usable(7),
	active(8) }

--  ImaLinkFailureStatus ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "Local failure status of a link belonging to an IMA group."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
--      SYNTAX      INTEGER {
--        noFailure(1),
--        imaLinkFailure(2),
--        lifFailure(3),
--        lodsFailure(4),
--        misConnected(5),
--        blocked(6),
--        fault(7),
--        farEndTxLinkUnusable(8),
--        farEndRxLinkUnusable(9) }
    ImaLinkFailureStatus ::= INTEGER {
	noFailure(1),
	imaLinkFailure(2),
	lifFailure(3),
	lodsFailure(4),
	misConnected(5),
	blocked(6),
	fault(7),
	farEndTxLinkUnusable(8),
	farEndRxLinkUnusable(9) }

--  ImaTestProcStatus ::= TEXTUAL-CONVENTION
--      STATUS      current
--      DESCRIPTION
--        "States of the Test Pattern Procedure."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 13 on page 81"
--      SYNTAX      INTEGER {
--        disabled(1),
--        operating(2),
--        linkFail(3) }
    ImaTestProcStatus ::= INTEGER {
	disabled(1),
	operating(2),
	linkFail(3) }

--
-- The IMA Group subtree
--
-- The IMA Group subtree consists of the number of IMA groups and a
-- table of IMA groups.  Each entry in the table of IMA groups contains
-- information (configuration and status) specific to each group.
--

imaGroupNumber OBJECT-TYPE
      SYNTAX      INTEGER (0..2147483647)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of IMA groups configured on this system."
      ::= { atmfImaMibObjects 1 }

imaGroupTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaGroupEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Group Configuration table."
      ::= { atmfImaMibObjects 2 }

imaGroupEntry OBJECT-TYPE
      SYNTAX      ImaGroupEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Group table."
      INDEX       { imaGroupIndex }
      ::= { imaGroupTable 1 }

ImaGroupEntry ::= SEQUENCE {
      imaGroupIndex               INTEGER (1..2147483647),
      imaGroupRowStatus           RowStatus,
      imaGroupIfIndex             InterfaceIndex,
      imaGroupNeState             ImaGroupState,
      imaGroupFeState             ImaGroupState,
      imaGroupFailureStatus       ImaGroupFailureStatus,
      imaGroupSymmetry            ImaGroupSymmetry,
      imaGroupMinNumTxLinks       INTEGER (1..32),
      imaGroupMinNumRxLinks       INTEGER (1..32),
      imaGroupNeTxClkMode         ImaGroupTxClkMode,
      imaGroupFeTxClkMode         ImaGroupTxClkMode,
      imaGroupTxTimingRefLink     InterfaceIndex,
      imaGroupRxTimingRefLink     InterfaceIndex,
      imaGroupLastChange          TimeTicks,
      imaGroupTxImaId             INTEGER (0..255),
      imaGroupRxImaId             INTEGER (0..255),
      imaGroupTxFrameLength       ImaFrameLength,
      imaGroupRxFrameLength       ImaFrameLength,
      imaGroupDiffDelayMax        MilliSeconds,
      imaGroupLeastDelayLink      InterfaceIndex,
      imaGroupDiffDelayMaxObs     MilliSeconds,
      imaGroupAlphaValue          INTEGER (1..2),
      imaGroupBetaValue           INTEGER (1..5),
      imaGroupGammaValue          INTEGER (1..5),
      imaGroupRunningSecs         Gauge32,
      imaGroupUnavailSecs         Counter32,
      imaGroupNeNumFailures       Counter32,
      imaGroupFeNumFailures       Counter32,
      imaGroupTxAvailCellRate     Gauge32,
      imaGroupRxAvailCellRate     Gauge32,
      imaGroupNumTxCfgLinks       Gauge32,
      imaGroupNumRxCfgLinks       Gauge32,
      imaGroupNumTxActLinks       Gauge32,
      imaGroupNumRxActLinks       Gauge32,
      imaGroupTestLinkIfIndex     InterfaceIndex,
      imaGroupTestPattern         INTEGER (-1..255),
      imaGroupTestProcStatus      ImaTestProcStatus,
      imaGroupValidIntervals      INTEGER (0..96),
      imaGroupInvalidIntervals    INTEGER (0..96),
      imaGroupTimeElapsed         INTEGER (0..899),
      imaGroupTxOamLabelValue     INTEGER (1..255),
      imaGroupRxOamLabelValue     INTEGER (0..255) }

imaGroupIndex OBJECT-TYPE
      SYNTAX      INTEGER (1..2147483647)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "A unique value for the IMA Group."
      ::= { imaGroupEntry 1 }

imaGroupRowStatus OBJECT-TYPE
      SYNTAX      RowStatus
      ACCESS      read-only
      STATUS      mandatory
          DESCRIPTION
        "The imaGroupRowStatus object allows create, change, and delete
        operations on imaGroupTable entries.

        To create a new conceptual row (or instance) of the imaGroupTable,
        imaGroupRowStatus must be set to 'createAndWait' or 'createAndGo'.
        If settable, a successful set of the following objects must be
        performed before the imaGroupRowStatus of a new conceptual row can
        be set to 'active':

          imaGroupMinNumTxLinks
          imaGroupMinNumRxLinks
          imaGroupTxImaId

        Some objects in the imaGroupTable control settings which can only
        be established or changed at group start-up time.  These objects
        include:

          imaGroupTxImaId
          imaGroupSymmetry
          imaGroupTxFrameLength

        To change (modify) the imaGroupTxImaId object, the manager must
        first set imaGroupRowStatus to 'notInService'.  However, changes
        to the following two objects can be optionally allowed while the
        imaGroupRowStatus is 'active':

          imaGroupSymmetry
          imaGroupTxFrameLength

        These two objects can be changed when the imaGroupRowStatus is
        'active' in order to allow the far-end to recover from its
        Config-Aborted state without having to force the near-end Group
        State machine to go to the 'Not Configured' state.  Changing
        these object values after group start-up has completed causes a
        restart of the IMA group.

        Alternatively, as noted above, the agent implementation may
        simply require the imaGroupRowStatus object to first be set to
        'notInService' before allowing changes to either of these two
        objects.

        To remove (delete) an imaGroupTable entry from this table, set
        imaGroupRowStatus to 'destroy'.

        Setting the imaGroupRowStatus to 'active' has the effect of
        activating the Group Startup Procedure.  The Group Startup
        Procedure uses provisioned links that have imaLinkRowStatus set
        to 'active' and imaLinkGroupIndex set to the imaGroupIndex in
        this conceptual row.

        When the imaGroupRowStatus is not in 'active' state, the Group
        State machine is in its 'Not Configured' state."
      ::= { imaGroupEntry 2 }

imaGroupIfIndex OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "This object identifies the logical interface number ('ifIndex')
        assigned to this IMA group, and is used to identify corresponding
        rows in the Interfaces MIB.

        Note that re-initialization of the management agent may cause
        a client's 'imaGroupIfIndex' to change."
      ::= { imaGroupEntry 3 }

imaGroupNeState OBJECT-TYPE
      SYNTAX      ImaGroupState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current operational state of the near-end IMA Group State
        Machine."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55"
      ::= { imaGroupEntry 4 }

imaGroupFeState OBJECT-TYPE
      SYNTAX      ImaGroupState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current operational state of the far-end IMA Group State
        Machine."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55"
      ::= { imaGroupEntry 5 }

imaGroupFailureStatus OBJECT-TYPE
      SYNTAX      ImaGroupFailureStatus
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current failure status of the IMA group (the reason why
        the GTSM is in the down state)."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55"
      ::= { imaGroupEntry 6 }

imaGroupSymmetry OBJECT-TYPE
      SYNTAX      ImaGroupSymmetry
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "Symmetry of the IMA group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.7 on page 35"
      DEFVAL { symmetricOperation }
      ::= { imaGroupEntry 7 }

imaGroupMinNumTxLinks OBJECT-TYPE
      SYNTAX      INTEGER (1..32)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "Minimum number of transmit links required to be Active for
        the IMA group to be in the Operational state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1.1 on page 55"
      ::= { imaGroupEntry 8 }

imaGroupMinNumRxLinks OBJECT-TYPE
      SYNTAX      INTEGER (1..32)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "Minimum number of receive links required to be Active for
        the IMA group to be in the Operational state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1.1 on page 55"
      ::= { imaGroupEntry 9 }

imaGroupNeTxClkMode OBJECT-TYPE
      SYNTAX      ImaGroupTxClkMode
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "Transmit clocking mode used by the near-end IMA group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 7 on page 38"
      DEFVAL { ctc }
      ::= { imaGroupEntry 10 }

imaGroupFeTxClkMode OBJECT-TYPE
      SYNTAX      ImaGroupTxClkMode
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Transmit clocking mode used by the far-end IMA group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 7 on page 38"
      ::= { imaGroupEntry 11 }

imaGroupTxTimingRefLink OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The ifIndex of the transmit timing reference link to be
        used by the near-end for IMA data cell clock recovery from
        the ATM layer.  The distinguished value of zero may be used
        if no link has been configured in the IMA group, or if the
        transmit timing reference link has not yet been selected."
      REFERENCE
        "ATM Forum IMA v1.1, Section 8.1.1 on page 41"
      ::= { imaGroupEntry 12 }

imaGroupRxTimingRefLink OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The ifIndex of the receive timing reference link to be
        used by near-end for IMA data cell clock recovery toward
        the ATM layer.  The distinguished value of zero may be used
        if no link has been configured in the IMA group, or if the
        receive timing reference link has not yet been detected."
      REFERENCE
        "ATM Forum IMA v1.1, Section 8.1.1 on page 41"
      ::= { imaGroupEntry 13 }

imaGroupLastChange OBJECT-TYPE
      SYNTAX      TimeTicks
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The time-of-day the IMA group last changed operational
        state (i.e., value of imaGroupNeState changed)."
      ::= { imaGroupEntry 14 }

imaGroupTxImaId OBJECT-TYPE
      SYNTAX      INTEGER (0..255)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "The IMA ID currently in use by the near-end IMA function."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.6 on page 35"
      ::= { imaGroupEntry 15 }

imaGroupRxImaId OBJECT-TYPE
      SYNTAX      INTEGER (0..255)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The IMA ID currently in use by the far-end IMA function."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.6 on page 35"
      ::= { imaGroupEntry 16 }

imaGroupTxFrameLength OBJECT-TYPE
      SYNTAX      ImaFrameLength
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "The frame length to be used by the IMA group in the transmit
        direction.  Can only be set when the IMA group is startup."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.4.2 on page 34"
      DEFVAL { m128 }
      ::= { imaGroupEntry 17 }

imaGroupRxFrameLength OBJECT-TYPE
      SYNTAX      ImaFrameLength
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Value of IMA frame length as received from remote IMA function."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.4.2 on page 34"
      ::= { imaGroupEntry 18 }

imaGroupDiffDelayMax OBJECT-TYPE
      SYNTAX      MilliSeconds
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "The maximum number of milliseconds of differential delay among
        the links that will be tolerated on this interface."
      REFERENCE
        "ATM Forum IMA v1.1, Section 9.2 on page 45"
      DEFVAL { 25 }
      ::= { imaGroupEntry 19 }

imaGroupLeastDelayLink OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The ifIndex of the link configured in the IMA group which has
        the smallest link propagation delay.  The distinguished value of
        zero may be used if no link has been configured in the IMA group,
        or if the link with the smallest link propagation delay has not
        yet been determined."
      REFERENCE
        "ATM Forum IMA v1.1, Section 9.2 on page 45"
      ::= { imaGroupEntry 20 }

imaGroupDiffDelayMaxObs OBJECT-TYPE
      SYNTAX      MilliSeconds
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The latest maximum differential delay observed (in milliseconds)
        between the links having the least and most link propagation delay,
        among the receive links that are currently configured in the IMA
        group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 9.2 on page 45"
      ::= { imaGroupEntry 21 }

imaGroupAlphaValue OBJECT-TYPE
      SYNTAX      INTEGER (1..2)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "This indicates the 'alpha' value used to specify the number
        of consecutive invalid ICP cells to be detected before moving
        to the IMA Hunt state from the IMA Sync state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 11 on page 68"
      DEFVAL { 2 }
      ::= { imaGroupEntry 22 }

imaGroupBetaValue OBJECT-TYPE
      SYNTAX      INTEGER (1..5)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "This indicates the 'beta' value used to specify the number
        of consecutive errored ICP cells to be detected before moving
        to the IMA Hunt state from the IMA Sync state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 11 on page 68"
      DEFVAL { 2 }
      ::= { imaGroupEntry 23 }

imaGroupGammaValue OBJECT-TYPE
      SYNTAX      INTEGER (1..5)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "This indicates the 'gamma' value used to specify the number
        of consecutive valid ICP cells to be detected before moving
        to the IMA Sync state from the IMA PreSync state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 11 on page 68"
      DEFVAL { 1 }
      ::= { imaGroupEntry 24 }

imaGroupRunningSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The amount of time (in seconds) since this IMA group has
        been in the Operational state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55"
      ::= { imaGroupEntry 25 }

imaGroupUnavailSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals where the IMA Group Traffic
        State Machine is Down."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55 and (R-136) in Section
        12.2.2.2 on page 77"
      ::= { imaGroupEntry 26 }

imaGroupNeNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end group failure (Config-Aborted,
        Insufficient-Links) has been reported since power-up or reboot."
      REFERENCE
        "ATM Forum IMA v1.1, (R-137) in Section 12.2.2.2 on page 77"
      ::= { imaGroupEntry 27 }

imaGroupFeNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end group failure (Config-Aborted-FE,
        Insufficient-Links-FE, Blocked-FE) has been reported since
        power-up or reboot.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-25) in Section 12.2.2.2 on page 77"
      ::= { imaGroupEntry 28 }

imaGroupTxAvailCellRate OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current cell rate (truncated value in cells per second)
        provided by this IMA group in the transmit direction,
        considering all the transmit links in the Active state."
      ::= { imaGroupEntry 29 }

imaGroupRxAvailCellRate OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current cell rate (truncated value in cells per second)
        provided by this IMA group in the receive direction,
        considering all the receive links in the Active state."
      ::= { imaGroupEntry 30 }

-- imaGroupNumTxCfgLinks is used by a network operator to tell how many
-- links are configured for transmit in the IMA group.

imaGroupNumTxCfgLinks OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of links that are configured to transmit in this IMA
        group. This attribute overwrites the value of the
        imaGroupNumRxActLinks attribute when the IMA group is configured
        in the Symmetrical Configuration group symmetry mode."
      ::= { imaGroupEntry 31 }

-- imaGroupNumRxCfgLinks is used by a network operator to tell how many
-- links are configured for receive in the IMA group.

imaGroupNumRxCfgLinks OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of links that are configured to receive in this IMA
        group. This attribute is overwritten by the value of the
        imaGroupNumTxActLinks attribute when the IMA group is configured
        in the Symmetrical Configuration group symmetry mode."
      ::= { imaGroupEntry 32 }

-- imaGroupNumTxActLinks is used by a network operator to tell how many
-- links which are configured for transmit are also Active.

imaGroupNumTxActLinks OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of links which are configured to transmit and are
        currently Active in this IMA group."
      ::= { imaGroupEntry 33 }

-- imaGroupNumRxActLinks is used by a network operator to tell how many
-- links which are configured for receive are also Active.

imaGroupNumRxActLinks OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of links which are configured to receive and are
        currently Active in this IMA group."
      ::= { imaGroupEntry 34 }

--
-- Test Pattern Procedure control objects.  These objects are implemented
-- if the IMA implements the Test Pattern Procedure.  In this case all
-- test pattern procedure related objects must be implemented.  Specifically,
-- these objects are:
--
--   imaGroupTestLinkIfIndex
--   imaGroupTestPattern
--   imaGroupTestProcStatus
--   imaLinkRxTestPattern
--   imaLinkTestProcStatus
--

imaGroupTestLinkIfIndex OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "This object is used to designate an interface as the test link
        for use in the Test Pattern Procedure.  The distinguished value of
        zero specifies that the implementation may choose the Test Link,
        in which case, the implementation may also choose the value of
        'imaGroupTestPattern'.  The value zero may also be used if no link
        has yet been added to the group.

        Note that this value is NOT the same as the Tx LID value, but
        instead either identifies the ifIndex value of the test link to be
        used by the Test Pattern Procedure (i.e., the link whose LID value
        is inserted in the Tx LID field of the transmitted ICP cells),
        or identifies that the implementation may choose the test link (if
        the value is zero)."
      REFERENCE
        "ATM Forum IMA v1.1, Section 13 on page 81"
      DEFVAL { 0 }
      ::= { imaGroupEntry 35 }

imaGroupTestPattern OBJECT-TYPE
      SYNTAX      INTEGER (-1..255)
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "The value of this object is used to specify the Tx Test Pattern
        in an IMA group loopback operation.  A value in the range 0 to
        255 designates a specific pattern.  The distinguished value of
        -1 specifies that the implementation may choose the value.  In
        this case, the implementation may also choose the value of
        'imaGroupTestLinkIfIndex'.

        It is recommended that the specific value 255 not be used for
        testing, since by (R-137) the IMA interface is required to
        transmit 0xFF (i.e., 255) when the incoming test command is
        inactive or the test link is not detected, and thus it cannot
        be established for certain whether 255 was received due to an
        actual loopback operation or due to the normal operation of an
        IMA that is not performing (or else cannot perform) the test
        pattern procedure."
      REFERENCE
        "ATM Forum IMA v1.1, Section 13 on page 81"
      DEFVAL { -1 }
      ::= { imaGroupEntry 36 }

imaGroupTestProcStatus OBJECT-TYPE
      SYNTAX      ImaTestProcStatus
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "This object is used to enable or disable the
        Test Pattern Procedure, and to note whether at least one
        link failed the test.

        The test is started by setting operating(2) status.  If any
        link should fail the test, the IMA will set the status to
        linkFail(3).  The linkFail(3) state will persist until
        either the disabled(1) state is set or until no instance
        of imaLinkTestProcStatus has the value linkFail(3).

        Only the values disabled(1) and operating(2) may be written.
        Writing the operating(2) value will not cause clearing of
        the linkFail(3) state."
      REFERENCE
        "ATM Forum IMA v1.1, Section 13 on page 81"
      DEFVAL { disabled }
      ::= { imaGroupEntry 37 }

--
-- Objects for use with the IMA Group Current Table, the IMA Group
-- Interval Table, and the IMA Group Total Table.
--
-- Implementation of these objects is optional, dependent on whether
-- the tables mentioned above are implemented.
--

imaGroupValidIntervals OBJECT-TYPE
      SYNTAX      INTEGER (0..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of previous 15 minute intervals for which valid data
        was collected.  The value will be 96 unless the IMA group table
        entry was created within the last 24 hours, in which case the value
        will be the number of complete 15 minute intervals since the IMA
        group table entry was created.  In the case where the agent is a
        proxy, it is possible that some intervals are unavailable.  In this
        case, this value is the maximum interval number for which valid
        data is available.  This attribute is only mandatory when the IMA
        Group Interval Statistics and/or IMA Group Total Statistics objects
        are implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaGroupEntry 38 }

imaGroupInvalidIntervals OBJECT-TYPE
      SYNTAX      INTEGER (0..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of intervals for which no valid data is available.
        This attribute is only mandatory when the IMA Group Interval
        Statistics and/or IMA Group Total Statistics objects are
        implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaGroupEntry 39 }

imaGroupTimeElapsed OBJECT-TYPE
      SYNTAX      INTEGER (0..899)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of seconds that have elapsed since the beginning of
        the current measurement period.  This attribute is only mandatory
        when the IMA Group Current Statistics are implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaGroupEntry 40 }

--
-- Objects to report the IMA OAM Label values transmitted and
-- received by the IMA group. 
--

imaGroupTxOamLabelValue OBJECT-TYPE
      SYNTAX      INTEGER (1..255)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "IMA OAM Label value transmitted by the NE IMA unit."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.3 on page 32"            
      ::= { imaGroupEntry 41 }

imaGroupRxOamLabelValue OBJECT-TYPE
      SYNTAX      INTEGER (0..255)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "IMA OAM Label value transmitted by the FE IMA unit.  The value 0
        likely means that the IMA unit has not received an OAM Label 
        from the FE IMA unit at this time."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.3 on page 32"
      ::= { imaGroupEntry 42 }

--
-- The IMA Group Mapping Table subtree
--
-- The IMA Group Mapping Table subtree consists of a table of mappings
-- from 'ifIndex' values of IMA groups to their 'imaGroupIndex' values.
-- This table allows the Unit Management to perform easy look-ups (no
-- searches and sorts).
--
-- Note that the Group Index is different than the ifIndex.
--

imaGroupMappingTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaGroupMappingEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "A table mapping the 'ifIndex' values of 'imaGroupIfIndex'
        to the 'imaGroupIndex' values of the corresponding IMA group."
      ::= { atmfImaMibObjects 3 }

imaGroupMappingEntry OBJECT-TYPE
      SYNTAX      ImaGroupMappingEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "Each row describes one ifIndex to imaGroupIndex mapping."
      INDEX       { ifIndex }
      ::= { imaGroupMappingTable 1 }

ImaGroupMappingEntry ::= SEQUENCE {
      imaGroupMappingIndex    Integer32 }

imaGroupMappingIndex OBJECT-TYPE
      SYNTAX      Integer32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The imaGroupIndex of the IMA Group which implements the
        specified interface."
      ::= { imaGroupMappingEntry 1 }

--
-- The IMA Link subtree
--
-- The IMA Link subtree consists of a table of IMA links.  Each entry
-- in the table contains status information about a link which is part
-- of an IMA group, and also contains a configuration object to select
-- to which IMA group the link belongs.
--

imaLinkTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaLinkEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA group Link Status and Configuration table."
      ::= { atmfImaMibObjects 4 }

imaLinkEntry OBJECT-TYPE
      SYNTAX      ImaLinkEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Group Link table."
      INDEX       { imaLinkIfIndex }
      ::= { imaLinkTable 1 }

ImaLinkEntry ::= SEQUENCE {
      imaLinkIfIndex              InterfaceIndex,
      imaLinkRowStatus            RowStatus,
      imaLinkGroupIndex           Integer32,
      imaLinkNeTxState            ImaLinkState,
      imaLinkNeRxState            ImaLinkState,
      imaLinkFeTxState            ImaLinkState,
      imaLinkFeRxState            ImaLinkState,
      imaLinkNeRxFailureStatus    ImaLinkFailureStatus,
      imaLinkFeRxFailureStatus    ImaLinkFailureStatus,
      imaLinkTxLid                INTEGER (0..31),
      imaLinkRxLid                INTEGER (0..31),
      imaLinkRelDelay             MilliSeconds,
      imaLinkImaViolations        Counter32,
      imaLinkOifAnomalies         Counter32,
      imaLinkNeSevErroredSecs     Counter32,
      imaLinkFeSevErroredSecs     Counter32,
      imaLinkNeUnavailSecs        Counter32,
      imaLinkFeUnavailSecs        Counter32,
      imaLinkNeTxUnusableSecs     Counter32,
      imaLinkNeRxUnusableSecs     Counter32,
      imaLinkFeTxUnusableSecs     Counter32,
      imaLinkFeRxUnusableSecs     Counter32,
      imaLinkNeTxNumFailures      Counter32,
      imaLinkNeRxNumFailures      Counter32,
      imaLinkFeTxNumFailures      Counter32,
      imaLinkFeRxNumFailures      Counter32,
      imaLinkTxStuffs             Counter32,
      imaLinkRxStuffs             Counter32,
      imaLinkRxTestPattern        INTEGER (0..255),
      imaLinkTestProcStatus       ImaTestProcStatus,
      imaLinkValidIntervals       INTEGER (0..96),
      imaLinkInvalidIntervals     INTEGER (0..96),
      imaLinkTimeElapsed          INTEGER (0..899) }

imaLinkIfIndex OBJECT-TYPE
      SYNTAX      InterfaceIndex
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "This corresponds to the 'ifIndex' of the MIB-II interface
        on which this link is established.  This object also
        corresponds to the logical number ('ifIndex') assigned to
        this IMA link."
      ::= { imaLinkEntry 1 }

imaLinkRowStatus OBJECT-TYPE
      SYNTAX      RowStatus
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The imaLinkRowStatus object allows create, change, and delete
        operations on imaLinkTable entries.

        To create a new conceptual row (or instance) of the imaLinkTable,
        imaLinkRowStatus must be set to 'createAndWait' or 'createAndGo'.
        A successful set of the imaLinkGroupIndex object must be performed
        before the imaLinkRowStatus of a new conceptual row can be set to
        'active'.

        To change (modify) the imaLinkGroupIndex in an imaLinkTable entry,
        the imaLinkRowStatus object must first be set to 'notInService'.
        Only then can this object in the conceptual row be modified.
        This is due to the fact that the imaLinkGroupIndex object provides
        the association between a physical IMA link and the IMA group to
        which it belongs, and setting the imaLinkGroupIndex object to a
        different value has the effect of changing the association between
        a physical IMA link and an IMA group.  To place the link 'in group',
        the imaLinkRowStatus object is set to 'active'.  While the row is
        not in 'active' state, both the Transmit and Receive IMA link state
        machines are in the 'Not In Group' state.

        To remove (delete) an imaLinkTable entry from this table, set
        this object to 'destroy'."
      ::= { imaLinkEntry 2 }

imaLinkGroupIndex OBJECT-TYPE
      SYNTAX      Integer32
      ACCESS      read-write
      STATUS      mandatory
      DESCRIPTION
        "The value which identifies the IMA group (imaGroupIndex)
        of which this link is a member."
      ::= { imaLinkEntry 3 }

imaLinkNeTxState OBJECT-TYPE
      SYNTAX      ImaLinkState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current state of the near-end transmit link."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 4 }

imaLinkNeRxState OBJECT-TYPE
      SYNTAX      ImaLinkState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current state of the near-end receive link."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 5 }

imaLinkFeTxState OBJECT-TYPE
      SYNTAX      ImaLinkState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current state of the far-end transmit link as reported
        via ICP cells."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 6 }

imaLinkFeRxState OBJECT-TYPE
      SYNTAX      ImaLinkState
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current state of the far-end receive link as reported
        via ICP cells."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 7 }

imaLinkNeRxFailureStatus OBJECT-TYPE
      SYNTAX      ImaLinkFailureStatus
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current link failure status of the near-end receive link."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 8 }

imaLinkFeRxFailureStatus OBJECT-TYPE
      SYNTAX      ImaLinkFailureStatus
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The current link failure status of the far-end receive link
        as reported via ICP cells."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.1.2 on page 48"
      ::= { imaLinkEntry 9 }

imaLinkTxLid OBJECT-TYPE
      SYNTAX      INTEGER (0..31)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The outgoing LID used currently on the link by the local end.
        This value has meaning only if the link belongs to an IMA group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.1 on page 26"
      ::= { imaLinkEntry 10 }

imaLinkRxLid OBJECT-TYPE
      SYNTAX      INTEGER (0..31)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The incoming LID used currently on the link by the remote
        end as reported via ICP cells.  This value has meaning only
        if the link belongs to an IMA group."
      REFERENCE
        "ATM Forum IMA v1.1, Section 5.2.2.1 on page 26"
      ::= { imaLinkEntry 11 }

imaLinkRelDelay OBJECT-TYPE
      SYNTAX      MilliSeconds
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The latest measured delay on this link relative to the link, in
        the same IMA group, with the least delay."
      REFERENCE
        "ATM Forum IMA v1.1, Section 9.2 on page 45"
      ::= { imaLinkEntry 12 }

imaLinkImaViolations OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "ICP violations: count of errored, invalid or missing ICP cells,
        except during SES-IMA or UAS-IMA conditions."
      REFERENCE
        "ATM Forum IMA v1.1, (R-125) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 13 }

imaLinkOifAnomalies OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of OIF anomalies, except during SES-IMA or UAS-IMA
        conditions, at the near-end.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-20) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 14 }

imaLinkNeSevErroredSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing >= 30% of the ICP cells
        counted as IV-IMAs, or one or more link defects (e.g., LOS, OOF/LOF,
        AIS, or LCD), LIF defects, or LODS defects, except during UAS-IMA
        condition."
      REFERENCE
        "ATM Forum IMA v1.1, (R-126) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 15 }

imaLinkFeSevErroredSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing one or more RDI-IMA
        defects, except during UAS-IMA-FE condition."
      REFERENCE
        "ATM Forum IMA v1.1, (R-127) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 16 }

imaLinkNeUnavailSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at near-end: unavailability begins
        at the onset of 10 contiguous SES-IMA and ends at the onset
        of 10 contiguous seconds with no SES-IMA."
      REFERENCE
        "ATM Forum IMA v1.1, (R-128) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 17 }

imaLinkFeUnavailSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at far-end: unavailability begins
        at the onset of 10 contiguous SES-IMA-FE and ends at the onset of
        10 contiguous seconds with no SES-IMA-FE."
      REFERENCE
        "ATM Forum IMA v1.1, (R-129) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 18 }

imaLinkNeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds: count of Tx Unusable seconds at the near-end
        Tx LSM."
      REFERENCE
        "ATM Forum IMA v1.1, (R-130) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 19 }

imaLinkNeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds: count of Rx Unusable seconds at the near-end
        Rx LSM."
      REFERENCE
        "ATM Forum IMA v1.1, (R-131) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 20 }

imaLinkFeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds at far-end: count of seconds with Tx Unusable
        indications from the far-end Tx LSM."
      REFERENCE
        "ATM Forum IMA v1.1, (R-132) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 21 }

imaLinkFeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds at far-end: count of seconds with Rx Unusable
        indications from the far-end Rx LSM."
      REFERENCE
        "ATM Forum IMA v1.1, (R-133) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 22 }

imaLinkNeTxNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end transmit failure alarm condition
        has been entered on this link (i.e., some form of implementation
        specific transmit fault)."
      REFERENCE
        "ATM Forum IMA v1.1, (R-134) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 23 }

imaLinkNeRxNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end receive failure alarm condition
        has been entered on this link (i.e., LIF, LODS, 
        RFI-IMA, Mis-Connected or some form of implementation specific receive
        fault)."
      REFERENCE
        "ATM Forum IMA v1.1, (R-135) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 24 }

imaLinkFeTxNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end transmit failure alarm condition
        has been entered on this link (i.e., Tx-Unusable-FE).  This is an
        optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-21) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 25 }

imaLinkFeRxNumFailures OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end receive failure alarm condition
        has been entered on this link (i.e., Rx-Unusable-FE).  This is an
        optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-22) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 26 }

imaLinkTxStuffs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events inserted in the transmit direction.
        This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-23) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 27 }

imaLinkRxStuffs OBJECT-TYPE
      SYNTAX      Counter32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events detected in the receive direction.
        This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-24) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 28 }

--
-- Test Pattern Procedure control objects.  These objects are implemented
-- if the IMA implements the Test Pattern Procedure.  In this case all
-- test pattern procedure related objects must be implemented.  Specifically,
-- these objects are:
--
--   imaGroupTestLinkIfIndex
--   imaGroupTestPattern
--   imaGroupTestProcStatus
--   imaLinkRxTestPattern
--   imaLinkTestProcStatus
--

imaLinkRxTestPattern OBJECT-TYPE
      SYNTAX      INTEGER (0..255)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "This object identifies the test pattern received in the
        ICP Cell (octet 17) on the link during the IMA Test Pattern
        Procedure.  This value may then be compared to the transmitted
        test pattern."
      ::= { imaLinkEntry 29 }

imaLinkTestProcStatus OBJECT-TYPE
      SYNTAX      ImaTestProcStatus
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "This value indicates the current state of the Test Pattern
        Procedure.  If the value is disabled(1), the test is not
        running.  A value of operating(2) means the test is running
        and no error has been found on this interface.  A value of
        linkFail(3) means an error has been detected on this link
        during the test.

        Once an error is detected, the linkFail(3) value is latched until
        either this object is read or until the imaGroupTestProcStatus
        is moved to disabled(1).  Once read, if the error no longer
        persists, a subsequent read will report the value operating(2)."
      ::= { imaLinkEntry 30 }

--
-- Objects for use with the IMA Link Current Table, the IMA Link
-- Interval Table, and the IMA Link Total Table.
--
-- Implementation of these objects is optional, dependent on whether
-- the tables mentioned above are implemented.
--

imaLinkValidIntervals OBJECT-TYPE
      SYNTAX      INTEGER (0..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of previous 15 minute intervals for which valid data
        was collected.  The value will be 96 unless the IMA group table
        entry was created within the last 24 hours, in which case the value
        will be the number of complete 15 minute intervals since the IMA
        group table entry was created.  In the case where the agent is a
        proxy, it is possible that some intervals are unavailable.  In this
        case, this value is the maximum interval number for which valid
        data is available.  This attribute is only mandatory when the IMA
        Link Interval Statistics and/or IMA Link Total Statistics objects
        are implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaLinkEntry 31 }

imaLinkInvalidIntervals OBJECT-TYPE
      SYNTAX      INTEGER (0..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of intervals for which no valid data is available.
        This attribute is only mandatory when the IMA Link Interval
        Statistics and/or IMA Link Total Statistics objects are
        implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 
         on page 77"
      ::= { imaLinkEntry 32 }

imaLinkTimeElapsed OBJECT-TYPE
      SYNTAX      INTEGER (0..899)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of seconds that have elapsed since the beginning of
        the current measurement period.  This attribute is only mandatory
        when the IMA Link Current Statistics are implemented."
      REFERENCE
        "ATM Forum IMA v1.1, (O-26) in Section 12.2.2.2 
         on page 77"
      ::= { imaLinkEntry 33 }

--
-- IMA Failure Alarms
--
-- Implementation of the imaFailureAlarm Trap is optional.
--

-- imaAlarmStatus OBJECT-TYPE
--      SYNTAX      ImaAlarmStatus
--      ACCESS      read-only
--      STATUS      mandatory
--      DESCRIPTION
--        "Status of the IMA alarm."
--       ::= { atmfImaMibObjects 5 }

-- imaAlarmType OBJECT-TYPE
--      SYNTAX      ImaAlarmType
--      ACCESS      read-only
--      STATUS      mandatory
--      DESCRIPTION
--        "The Type of IMA alarm declared or cleared.  The value of
--        ImaAlarmType identifies the type of alarm according to the
--        definitions in the IMA specification."
--      REFERENCE
--        "ATM Forum IMA v1.1, Section 12.2.3 on page 79"
--       ::= { atmfImaMibObjects 6 }

--imaFailureAlarm NOTIFICATION-TYPE
--      OBJECTS {
--        ifIndex,
--        imaAlarmStatus,
--        imaAlarmType }
--      STATUS      mandatory
--      ::= { atmfImaMibTrapPrefix 1 }

--
-- The IMA Group Current Statistics subtree
--
-- The IMA Group Current Statistics subtree consists of a single table:
-- the IMA Group Current Table.  This table contains various statistics
-- collected by each IMA group for the current 15 minute interval.
--
-- Implementation of IMA Group Current Table is optional.
--

imaGroupCurrentTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaGroupCurrentEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Group Current table."
      ::= { atmfImaMibObjects 7 }

imaGroupCurrentEntry OBJECT-TYPE
      SYNTAX      ImaGroupCurrentEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Group Current table."
      INDEX       { imaGroupIndex }
      ::= { imaGroupCurrentTable 1 }

ImaGroupCurrentEntry ::= SEQUENCE {
      imaGroupCurrentUnavailSecs     Gauge32,
      imaGroupCurrentNeNumFailures   Gauge32,
      imaGroupCurrentFeNumFailures   Gauge32 }

imaGroupCurrentUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals where the IMA Group Traffic
        State Machine is Down in the current 15 minutes interval."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55, (R-136) and
        (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaGroupCurrentEntry 1 }

imaGroupCurrentNeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end group failure (Config-Aborted,
        Insufficient-Links) has been reported in the current 15
        minutes interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-137) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaGroupCurrentEntry 2 }

imaGroupCurrentFeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end group failure (Config-Aborted-FE,
        Insufficient-Links-FE, Blocked-FE) has been reported in the
        current 15 minutes interval.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-25) and (O-26) in Section 12.2.2.2
        on page 77"
      ::= { imaGroupCurrentEntry 3 }

--
-- The IMA Group Interval Statistics subtree
--
-- The IMA Group Interval Statistics subtree consists of a single table:
-- the IMA Group Interval Table.  This table contains various statistics
-- collected by each IMA group over the previous 24 hours of operation.
-- The past 24 hours are broken into 96 completed 15 minute intervals.
--
-- Implementation of IMA Group Interval Table is optional.
--

imaGroupIntervalTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaGroupIntervalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Group Interval table."
      ::= { atmfImaMibObjects 8 }

imaGroupIntervalEntry OBJECT-TYPE
      SYNTAX      ImaGroupIntervalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Group Interval table."
      INDEX       { imaGroupIndex, imaGroupIntervalNumber }
      ::= { imaGroupIntervalTable 1 }

ImaGroupIntervalEntry ::= SEQUENCE {
      imaGroupIntervalNumber          INTEGER (1..96),
      imaGroupIntervalUnavailSecs     Gauge32,
      imaGroupIntervalNeNumFailures   Gauge32,
      imaGroupIntervalFeNumFailures   Gauge32 }

imaGroupIntervalNumber OBJECT-TYPE
      SYNTAX      INTEGER (1..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "A number between 1 and 96, where 1 is the most
         recently completed 15 minute interval and 96 is the least
         recently completed 15 minutes interval (assuming that all
         96 intervals are valid)."
      ::= { imaGroupIntervalEntry 1 }

imaGroupIntervalUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals where the IMA Group Traffic
        State Machine is Down in one of the previous 96, individual 15
        minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55, (R-136) and 
        (O-26) in Section 12.2.2.2 on page 77"
      ::= { imaGroupIntervalEntry 2 }

imaGroupIntervalNeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end group failure (Config-Aborted,
        Insufficient-Links) has been reported in one of the previous
        96, individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-137) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaGroupIntervalEntry 3 }

imaGroupIntervalFeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end group failure (Config-Aborted-FE,
        Insufficient-Links-FE, Blocked-FE) has been reported in one of
        the previous 96, individual 15 minute, intervals.  This is an
        optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-25) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaGroupIntervalEntry 4 }

--
-- The IMA Group Total Statistics subtree
--
-- The IMA Group Total Statistics subtree consists of a single table:
-- the IMA Group Total Table.  This table contains the cumulative sum
-- of the various statistics collected by each IMA group for the 24 hour
-- period preceding the current interval.
--
-- Implementation of IMA Group Total Table is optional.
--

imaGroupTotalTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaGroupTotalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Group Total table."
      ::= { atmfImaMibObjects 9 }

imaGroupTotalEntry OBJECT-TYPE
      SYNTAX      ImaGroupTotalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Group Total table."
      INDEX       { imaGroupIndex }
      ::= { imaGroupTotalTable 1 }

ImaGroupTotalEntry ::= SEQUENCE {
      imaGroupTotalUnavailSecs     Gauge32,
      imaGroupTotalNeNumFailures   Gauge32,
      imaGroupTotalFeNumFailures   Gauge32 }

imaGroupTotalUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals where the IMA Group Traffic
        State Machine is Down in the previous 24 hour interval.
        Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, Section 10.2.1 on page 55, (R-136) and 
        (O-27) in Section 12.2.2.2 on page 77"
      ::= { imaGroupTotalEntry 1 }

imaGroupTotalNeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end group failure (Config-Aborted,
        Insufficient-Links) has been reported in the previous 24 hour
        interval.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-137) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaGroupTotalEntry 2 }

imaGroupTotalFeNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end group failure (Config-Aborted-FE,
        Insufficient-Links-FE, Blocked-FE) has been reported in the
        previous 24 hour interval.  Invalid 15 minute intervals count
        as 0.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-25) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaGroupTotalEntry 3 }

--
-- The IMA Link Current Statistics subtree
--
-- The IMA Link Current Statistics subtree consists of a single table:
-- the IMA Link Current Table.  This table contains various statistics
-- collected by each IMA link for the current 15 minute interval.
--
-- Implementation of IMA Link Current Table is optional.
--

imaLinkCurrentTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaLinkCurrentEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Link Current table."
      ::= { atmfImaMibObjects 10 }

imaLinkCurrentEntry OBJECT-TYPE
      SYNTAX      ImaLinkCurrentEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Link Current table."
      INDEX       { ifIndex }
      ::= { imaLinkCurrentTable 1 }

ImaLinkCurrentEntry ::= SEQUENCE {
      imaLinkCurrentImaViolations     Gauge32,
      imaLinkCurrentOifAnomalies      Gauge32,
      imaLinkCurrentNeSevErroredSecs  Gauge32,
      imaLinkCurrentFeSevErroredSecs  Gauge32,
      imaLinkCurrentNeUnavailSecs     Gauge32,
      imaLinkCurrentFeUnavailSecs     Gauge32,
      imaLinkCurrentNeTxUnusableSecs  Gauge32,
      imaLinkCurrentNeRxUnusableSecs  Gauge32,
      imaLinkCurrentFeTxUnusableSecs  Gauge32,
      imaLinkCurrentFeRxUnusableSecs  Gauge32,
      imaLinkCurrentNeTxNumFailures   Gauge32,
      imaLinkCurrentNeRxNumFailures   Gauge32,
      imaLinkCurrentFeTxNumFailures   Gauge32,
      imaLinkCurrentFeRxNumFailures   Gauge32,
      imaLinkCurrentTxStuffs          Gauge32,
      imaLinkCurrentRxStuffs          Gauge32 }

imaLinkCurrentImaViolations OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "ICP violations: count of errored, invalid or missing ICP cells,
        except during SES-IMA or UAS-IMA conditions, in the current
        15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-125) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 1 }

imaLinkCurrentOifAnomalies OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of OIF anomalies, except during SES-IMA or UAS-IMA
        conditions, at the near-end in the current 15 minute interval.
        This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-20) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 2 }

imaLinkCurrentNeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing >= 30% of the ICP cells
        counted as IV-IMAs, or one or more link defects (e.g., LOS, OOF/LOF,
        AIS, or LCD), LIF defects, or LODS defects, except during UAS-IMA
        condition, in the current 15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-126) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 3 }

imaLinkCurrentFeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing one or more RDI-IMA
        defects, except during UAS-IMA-FE condition, in the current 15
        minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-127) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 4 }

imaLinkCurrentNeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at near-end in the current 15 minute
        interval: unavailability begins at the onset of 10 contiguous
        SES-IMA and ends at the onset of 10 contiguous seconds with no
        SES-IMA."
      REFERENCE
        "ATM Forum IMA v1.1, (R-128) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 5 }

imaLinkCurrentFeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at far-end in the current 15 minute
        interval: unavailability begins at the onset of 10 contiguous
        SES-IMA-FE and ends at the onset of 10 contiguous seconds with no
        SES-IMA-FE."
      REFERENCE
        "ATM Forum IMA v1.1, (R-129) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 6 }

imaLinkCurrentNeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds: count of Unusable seconds at the near-end
        Tx LSM in the current 15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-130) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 7 }

imaLinkCurrentNeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds: count of Unusable seconds at the near-end
        Rx LSM in the current 15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-131) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 8 }

imaLinkCurrentFeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds at far-end: count of seconds with Tx Unusable
        indications from the far-end Tx LSM in the current 15 minute
        interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-132) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 9 }

imaLinkCurrentFeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds at far-end: count of seconds with Rx Unusable
        indications from the far-end Rx LSM in the current 15 minute
        interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-133) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 10 }

imaLinkCurrentNeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end transmit failure alarm condition
        has been entered on this link (i.e., some form of implementation
        specific transmit fault) in the current 15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-134) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 11 }

imaLinkCurrentNeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end receive failure alarm condition
        has been entered on this link (i.e., LIF, LODS, RFI-IMA, Mis-Connected,
        or some form of implementation specific receive fault)
        in the current 15 minute interval."
      REFERENCE
        "ATM Forum IMA v1.1, (R-135) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 12 }

imaLinkCurrentFeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end transmit failure alarm condition
        has been entered on this link (i.e., Tx-Unusable-FE) in the
        current 15 minute interval.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-21) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 13 }

imaLinkCurrentFeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end receive failure alarm condition
        has been entered on this link (i.e., Rx-Unusable-FE) in the
        current 15 minute interval.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-22) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 14 }

imaLinkCurrentTxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events inserted in the transmit direction in
        the current 15 minute interval.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-23) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 15 }

imaLinkCurrentRxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events detected in the receive direction in
        the current 15 minute interval.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-24) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkCurrentEntry 16 }

--
-- The IMA Link Interval Statistics subtree
--
-- The IMA Link Interval Statistics subtree consists of a single table:
-- the IMA Link Interval Table.  This table contains various statistics
-- collected by each IMA link over the previous 24 hours of operation.
-- The past 24 hours are broken into 96 completed 15 minute intervals.
--
-- Implementation of IMA Link Interval Table is optional.
--

imaLinkIntervalTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaLinkIntervalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Link Interval table."
      ::= { atmfImaMibObjects 11 }

imaLinkIntervalEntry OBJECT-TYPE
      SYNTAX      ImaLinkIntervalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Link Interval table."
      INDEX       { ifIndex, imaLinkIntervalNumber }
      ::= { imaLinkIntervalTable 1 }

ImaLinkIntervalEntry ::= SEQUENCE {
      imaLinkIntervalNumber            INTEGER (1..96),
      imaLinkIntervalImaViolations     Gauge32,
      imaLinkIntervalOifAnomalies      Gauge32,
      imaLinkIntervalNeSevErroredSecs  Gauge32,
      imaLinkIntervalFeSevErroredSecs  Gauge32,
      imaLinkIntervalNeUnavailSecs     Gauge32,
      imaLinkIntervalFeUnavailSecs     Gauge32,
      imaLinkIntervalNeTxUnusableSecs  Gauge32,
      imaLinkIntervalNeRxUnusableSecs  Gauge32,
      imaLinkIntervalFeTxUnusableSecs  Gauge32,
      imaLinkIntervalFeRxUnusableSecs  Gauge32,
      imaLinkIntervalNeTxNumFailures   Gauge32,
      imaLinkIntervalNeRxNumFailures   Gauge32,
      imaLinkIntervalFeTxNumFailures   Gauge32,
      imaLinkIntervalFeRxNumFailures   Gauge32,
      imaLinkIntervalTxStuffs          Gauge32,
      imaLinkIntervalRxStuffs          Gauge32 }

imaLinkIntervalNumber OBJECT-TYPE
      SYNTAX      INTEGER (1..96)
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "A number between 1 and 96, where 1 is the most
         recently completed 15 minute interval and 96 is the least
         recently completed 15 minutes interval (assuming that all
         96 intervals are valid)."
      ::= { imaLinkIntervalEntry 1 }

imaLinkIntervalImaViolations OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "ICP violations: count of errored, invalid or missing ICP cells,
        except during SES-IMA or UAS-IMA conditions, in one of the
        previous 96, individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-125) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 2 }

imaLinkIntervalOifAnomalies OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of OIF anomalies, except during SES-IMA or UAS-IMA
        conditions, at the near-end in one of the previous 96, individual
        15 minute, intervals.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-20) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 3 }

imaLinkIntervalNeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing >= 30% of the ICP cells
        counted as IV-IMAs, or one or more link defects (e.g., LOS, OOF/LOF,
        AIS, or LCD), LIF defects, or LODS defects, except during UAS-IMA
        condition, in one of the previous 96, individual 15 minute,
        intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-126) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 4 }

imaLinkIntervalFeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing one or more RDI-IMA
        defects, except during UAS-IMA-FE condition, in one of the previous
        96, individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-127) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 5 }

imaLinkIntervalNeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at near-end in one of the previous
        96, individual 15 minute, intervals: unavailability begins at the
        onset of 10 contiguous SES-IMA and ends at the onset of 10
        contiguous seconds with no SES-IMA."
      REFERENCE
        "ATM Forum IMA v1.1, (R-128) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 6 }

imaLinkIntervalFeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at far-end in one of the previous
        96, individual 15 minute, intervals: unavailability begins at the
        onset of 10 contiguous SES-IMA-FE and ends at the onset of 10
        contiguous seconds with no SES-IMA-FE."
      REFERENCE
        "ATM Forum IMA v1.1, (R-129) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 7 }

imaLinkIntervalNeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds: count of Unusable seconds at the near-end
        Tx LSM in one of the previous 96, individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-130) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 8 }

imaLinkIntervalNeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds: count of Unusable seconds at the near-end
        Rx LSM in one of the previous 96, individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-131) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 9 }

imaLinkIntervalFeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds at far-end: count of seconds with Tx Unusable
        indications from the far-end Tx LSM in one of the previous 96,
        individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-132) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 10 }

imaLinkIntervalFeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds at far-end: count of seconds with Rx Unusable
        indications from the far-end Rx LSM in one of the previous 96,
        individual 15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-133) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 11 }

imaLinkIntervalNeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end transmit failure alarm condition
        has been entered on this link (i.e., some form of implementation
        specific transmit fault) in one of the previous 96, individual
        15 minute, intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-134) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 12 }

imaLinkIntervalNeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end receive failure alarm condition
        has been entered on this link (i.e., LIF, LODS, RFI-IMA, 
        Mis-Connected, or some form of implementation specific 
        receive fault) in one of the previous 96, individual 15 minute,
        intervals."
      REFERENCE
        "ATM Forum IMA v1.1, (R-135) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 13 }

imaLinkIntervalFeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end transmit failure alarm condition
        has been entered on this link (i.e., Tx-Unusable-FE) in one of the
        previous 96, individual 15 minute, intervals.  This is an optional
        attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-21) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 14 }

imaLinkIntervalFeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end receive failure alarm condition
        has been entered on this link (i.e., Rx-Unusable-FE) in one of
        the previous 96, individual 15 minute, intervals.  This is an
        optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-22) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 15 }

imaLinkIntervalTxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events inserted in the transmit direction in
        one of the previous 96, individual 15 minute, intervals.  This
        is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-23) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 16 }

imaLinkIntervalRxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events detected in the receive direction in
        one of the previous 96, individual 15 minute, intervals.  This
        is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-24) and (O-26) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkIntervalEntry 17 }

--
-- The IMA Link Total Statistics subtree
--
-- The IMA Link Total Statistics subtree consists of a single table:
-- the IMA Link Total Table.  This table contains the cumulative sum
-- of the various statistics collected by each IMA link for the 24 hour
-- period preceding the current interval.
--
-- Implementation of IMA Link Total Table is optional.
--

imaLinkTotalTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ImaLinkTotalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "The IMA Link Total table."
      ::= { atmfImaMibObjects 12 }

imaLinkTotalEntry OBJECT-TYPE
      SYNTAX      ImaLinkTotalEntry
      ACCESS      not-accessible
      STATUS      mandatory
      DESCRIPTION
        "An entry in the IMA Link Total table."
      INDEX       { ifIndex }
      ::= { imaLinkTotalTable 1 }

ImaLinkTotalEntry ::= SEQUENCE {
      imaLinkTotalImaViolations     Gauge32,
      imaLinkTotalOifAnomalies      Gauge32,
      imaLinkTotalNeSevErroredSecs  Gauge32,
      imaLinkTotalFeSevErroredSecs  Gauge32,
      imaLinkTotalNeUnavailSecs     Gauge32,
      imaLinkTotalFeUnavailSecs     Gauge32,
      imaLinkTotalNeTxUnusableSecs  Gauge32,
      imaLinkTotalNeRxUnusableSecs  Gauge32,
      imaLinkTotalFeTxUnusableSecs  Gauge32,
      imaLinkTotalFeRxUnusableSecs  Gauge32,
      imaLinkTotalNeTxNumFailures   Gauge32,
      imaLinkTotalNeRxNumFailures   Gauge32,
      imaLinkTotalFeTxNumFailures   Gauge32,
      imaLinkTotalFeRxNumFailures   Gauge32,
      imaLinkTotalTxStuffs          Gauge32,
      imaLinkTotalRxStuffs          Gauge32 }

imaLinkTotalImaViolations OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "ICP violations: count of errored, invalid or missing ICP cells,
        except during SES-IMA or UAS-IMA conditions, in the previous 24
        hour interval.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-125) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 1 }

imaLinkTotalOifAnomalies OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of OIF anomalies, except during SES-IMA or UAS-IMA
        conditions, at the near-end in the previous 24 hour interval.
        Invalid 15 minute intervals count as 0.  This is an optional
        attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-20) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 2 }

imaLinkTotalNeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing >= 30% of the ICP cells
        counted as IV-IMAs, or one or more link defects (e.g., LOS, OOF/LOF,
        AIS, or LCD), LIF defects, or LODS defects, except during UAS-IMA
        condition, in the previous 24 hour interval.  Invalid 15 minute
        intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-126) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 3 }

imaLinkTotalFeSevErroredSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of one second intervals containing one or more RDI-IMA
        defects, except during UAS-IMA-FE condition, in the previous 24
        hour interval.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-127) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 4 }

imaLinkTotalNeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at near-end in the previous 24 hour
        interval: unavailability begins at the onset of 10 contiguous
        SES-IMA and ends at the onset of 10 contiguous seconds with no
        SES-IMA.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-128) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 5 }

imaLinkTotalFeUnavailSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of unavailable seconds at far-end in the previous 24 hour
        interval: unavailability begins at the onset of 10 contiguous
        SES-IMA-FE and ends at the onset of 10 contiguous seconds with no
        SES-IMA-FE.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-129) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 6 }

imaLinkTotalNeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds: count of Unusable seconds at the near-end
        Tx LSM in the previous 24 hour interval.  Invalid 15 minute
        intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-130) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 7 }

imaLinkTotalNeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds: count of Unusable seconds at the near-end
        Rx LSM in the previous 24 hour interval.  Invalid 15 minute
        intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-131) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 8 }

imaLinkTotalFeTxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Tx Unusable seconds at far-end: count of seconds with Tx Unusable
        indications from the far-end Tx LSM in the previous 24 hour
        interval.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-132) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 9 }

imaLinkTotalFeRxUnusableSecs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Rx Unusable seconds at far-end: count of seconds with Rx Unusable
        indications from the far-end Rx LSM in the previous 24 hour
        interval.  Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-133) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 10 }

imaLinkTotalNeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end transmit failure alarm condition
        has been entered on this link (i.e., some form of implementation
        specific transmit fault) in the previous 24 hour interval.
        Invalid 15 minute intervals count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-134) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 11 }

imaLinkTotalNeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a near-end receive failure alarm condition
        has been entered on this link (i.e., LIF, LODS, RFI-IMA, 
        Mis-Connected, or some form of implementation specific receive fault)
        in the previous 24 hour interval. Invalid 15 minute intervals
        count as 0."
      REFERENCE
        "ATM Forum IMA v1.1, (R-135) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 12 }

imaLinkTotalFeTxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end transmit failure alarm condition
        has been entered on this link (i.e., Tx-Unusable-FE) in the
        previous 24 hour interval.  Invalid 15 minute intervals count
        as 0.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-21) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 13 }

imaLinkTotalFeRxNumFailures OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "The number of times a far-end receive failure alarm condition
        has been entered on this link (i.e., Rx-Unusable-FE) in the
        previous 24 hour interval.  Invalid 15 minute intervals count
        as 0.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-22) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 14 }

imaLinkTotalTxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events inserted in the transmit direction in
        the previous 24 hour interval.  Invalid 15 minute intervals
        count as 0.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-23) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 15 }

imaLinkTotalRxStuffs OBJECT-TYPE
      SYNTAX      Gauge32
      ACCESS      read-only
      STATUS      mandatory
      DESCRIPTION
        "Count of stuff events detected in the receive direction in
        the previous 24 hour interval.  Invalid 15 minute intervals
        count as 0.  This is an optional attribute."
      REFERENCE
        "ATM Forum IMA v1.1, (O-24) and (O-27) in Section 12.2.2.2 
        on page 77"
      ::= { imaLinkTotalEntry 16 }

-- Conformance Information

--  atmfImaMibGroups OBJECT IDENTIFIER ::= { atmfImaMibConformance 1 }
--  atmfImaMibCompliances OBJECT IDENTIFIER ::= { atmfImaMibConformance 2 }

-- Compliance Statements

--  atmfImaMibCompliance MODULE-COMPLIANCE
--      STATUS      mandatory
--      DESCRIPTION
--        "The compliance statement for network elements implementing
--        ATM Forum Inverse Multiplexing for ATM (IMA) interfaces."
--      MODULE -- this module

-- Mandatory Part

--      MANDATORY-GROUPS {
--        imaGroupGroup,
--        imaLinkGroup,
--        imaGroupMappingTableGroup,
--        imaAlarmGroup,
--        imaNotificationsGroup }

--      GROUP imaTestPatternGroup
--      DESCRIPTION
--        "This group is mandatory only for implementations that support
--        the Test Pattern Procedure."

--      GROUP imaGroupIntervalGroup
--      DESCRIPTION
--        "This group is mandatory only for implementations that support
--        interval statistics."

--      GROUP imaLinkIntervalGroup
--      DESCRIPTION
--        "This group is mandatory only for implementations that support
--        interval statistics."

-- Compliance Part

--      OBJECT imaGroupSymmetry
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupMinNumTxLinks
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupMinNumRxLinks
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupTxImaId
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupTxFrameLength
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupDiffDelayMax
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupAlphaValue
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupBetaValue
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupGammaValue
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupFeNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaGroupTestLinkIfIndex
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaGroupTestPattern
--      MIN-ACCESS read-only
--      DESCRIPTION
--        "Write access is not required."

--      OBJECT imaLinkOifAnomalies
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkFeTxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkFeRxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkRxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaGroupCurrentFeNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaGroupIntervalFeNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaGroupTotalFeNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkCurrentOifAnomalies
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkCurrentFeTxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkCurrentFeRxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkCurrentTxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkCurrentRxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkIntervalOifAnomalies
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkIntervalFeTxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkIntervalFeRxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkIntervalTxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkIntervalRxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTotalOifAnomalies
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTotalFeTxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTotalFeRxNumFailures
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTotalTxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--      OBJECT imaLinkTotalRxStuffs
--      MIN-ACCESS not-accessible
--      DESCRIPTION
--        "This is an optional attribute."

--   ::= { atmfImaMibCompliances 1 }

-- Units of Conformance

--  imaGroupGroup OBJECT-GROUP
--      OBJECTS {
--        imaGroupNumber,
--        imaGroupRowStatus,
--        imaGroupIfIndex,
--        imaGroupNeState,
--        imaGroupFeState,
--        imaGroupFailureStatus,
--        imaGroupSymmetry,
--        imaGroupMinNumTxLinks,
--        imaGroupMinNumRxLinks,
--        imaGroupNeTxClkMode,
--        imaGroupFeTxClkMode,
--        imaGroupTxTimingRefLink,
--        imaGroupRxTimingRefLink,
--        imaGroupLastChange,
--        imaGroupTxImaId,
--        imaGroupRxImaId,
--        imaGroupTxFrameLength,
--        imaGroupRxFrameLength,
--        imaGroupDiffDelayMax,
--        imaGroupLeastDelayLink,
--        imaGroupDiffDelayMaxObs,
--        imaGroupAlphaValue,
--        imaGroupBetaValue,
--        imaGroupGammaValue,
--        imaGroupRunningSecs,
--        imaGroupUnavailSecs,
--        imaGroupNeNumFailures,
--        imaGroupFeNumFailures,
--        imaGroupTxAvailCellRate,
--        imaGroupRxAvailCellRate,
--        imaGroupNumTxCfgLinks,
--        imaGroupNumRxCfgLinks,
--        imaGroupNumTxActLinks,
--        imaGroupNumRxActLinks,
--        imaGroupTxOamLabelValue,
--        imaGroupRxOamLabelValue }
--      STATUS     mandatory
--      DESCRIPTION
--        "A set of objects providing configuration and status information for
--        an IMA group definition."
--      ::= { atmfImaMibGroups 1 }

--  imaLinkGroup OBJECT-GROUP
--      OBJECTS {
--        imaLinkRowStatus,
--        imaLinkGroupIndex,
--        imaLinkNeTxState,
--        imaLinkNeRxState,
--        imaLinkFeTxState,
--        imaLinkFeRxState,
--        imaLinkNeRxFailureStatus,
--        imaLinkFeRxFailureStatus,
--        imaLinkTxLid,
--        imaLinkRxLid,
--        imaLinkRelDelay,
--        imaLinkImaViolations,
--        imaLinkOifAnomalies,
--        imaLinkNeSevErroredSecs,
--        imaLinkFeSevErroredSecs,
--        imaLinkNeUnavailSecs,
--        imaLinkFeUnavailSecs,
--        imaLinkNeTxUnusableSecs,
--        imaLinkNeRxUnusableSecs,
--        imaLinkFeTxUnusableSecs,
--        imaLinkFeRxUnusableSecs,
--        imaLinkNeTxNumFailures,
--        imaLinkNeRxNumFailures,
--        imaLinkFeTxNumFailures,
--        imaLinkFeRxNumFailures,
--        imaLinkTxStuffs,
--        imaLinkRxStuffs }
--      STATUS     mandatory
--      DESCRIPTION
--        "A set of objects providing status information for an IMA link."
--      ::= { atmfImaMibGroups 2 }

--  imaGroupMappingTableGroup OBJECT-GROUP
--      OBJECTS {
--        imaGroupMappingIndex }
--      STATUS     mandatory
--      DESCRIPTION
--        "A table mapping the 'ifIndex' values of 'imaGroupIfIndex'
--        to the 'imaGroupIndex' values of the corresponding
--        IMA group."
--      ::= { atmfImaMibGroups 3 }

--  imaTestPatternGroup OBJECT-GROUP
--      OBJECTS {
--        imaGroupTestLinkIfIndex,
--        imaGroupTestPattern,
--        imaGroupTestProcStatus,
--        imaLinkRxTestPattern,
--        imaLinkTestProcStatus }
--      STATUS     mandatory
--      DESCRIPTION
--        "Objects in the imaGroupTable and imaLinkTable which control and
--        report on the Test Pattern Procedure.  These objects must be
--        implemented if the IMA Test Pattern Procedure is supported."
--      ::= { atmfImaMibGroups 4 }

--  imaAlarmGroup OBJECT-GROUP
--      OBJECTS {
--        imaAlarmStatus,
--        imaAlarmType }
--      STATUS     mandatory
--      DESCRIPTION
--        "Objects used in the imaFailureAlarm notification."
--      ::= { atmfImaMibGroups 5 }

--  imaGroupIntervalGroup OBJECT-GROUP
--      OBJECTS {
--        imaGroupValidIntervals,
--        imaGroupInvalidIntervals,
--        imaGroupTimeElapsed,
--        imaGroupCurrentUnavailSecs,
--        imaGroupCurrentNeNumFailures,
--        imaGroupCurrentFeNumFailures,
--        imaGroupIntervalUnavailSecs,
--        imaGroupIntervalNeNumFailures,
--        imaGroupIntervalFeNumFailures,
--        imaGroupTotalUnavailSecs,
--        imaGroupTotalNeNumFailures,
--        imaGroupTotalFeNumFailures }
--      STATUS     mandatory
--      DESCRIPTION
--        "Objects containing interval statistics for an IMA group."
--      ::= { atmfImaMibGroups 6 }

--  imaLinkIntervalGroup OBJECT-GROUP
--      OBJECTS {
--        imaLinkValidIntervals,
--        imaLinkInvalidIntervals,
--        imaLinkTimeElapsed,
--        imaLinkCurrentImaViolations,
--        imaLinkCurrentOifAnomalies,
--        imaLinkCurrentNeSevErroredSecs,
--        imaLinkCurrentFeSevErroredSecs,
--        imaLinkCurrentNeUnavailSecs,
--        imaLinkCurrentFeUnavailSecs,
--        imaLinkCurrentNeTxUnusableSecs,
--        imaLinkCurrentNeRxUnusableSecs,
--        imaLinkCurrentFeTxUnusableSecs,
--        imaLinkCurrentFeRxUnusableSecs,
--        imaLinkCurrentNeTxNumFailures,
--        imaLinkCurrentNeRxNumFailures,
--        imaLinkCurrentFeTxNumFailures,
--        imaLinkCurrentFeRxNumFailures,
--        imaLinkCurrentTxStuffs,
--        imaLinkCurrentRxStuffs,
--        imaLinkIntervalImaViolations,
--        imaLinkIntervalOifAnomalies,
--        imaLinkIntervalNeSevErroredSecs,
--        imaLinkIntervalFeSevErroredSecs,
--        imaLinkIntervalNeUnavailSecs,
--        imaLinkIntervalFeUnavailSecs,
--        imaLinkIntervalNeTxUnusableSecs,
--        imaLinkIntervalNeRxUnusableSecs,
--        imaLinkIntervalFeTxUnusableSecs,
--        imaLinkIntervalFeRxUnusableSecs,
--        imaLinkIntervalNeTxNumFailures,
--        imaLinkIntervalNeRxNumFailures,
--        imaLinkIntervalFeTxNumFailures,
--        imaLinkIntervalFeRxNumFailures,
--        imaLinkIntervalTxStuffs,
--        imaLinkIntervalRxStuffs,
--        imaLinkTotalImaViolations,
--        imaLinkTotalOifAnomalies,
--        imaLinkTotalNeSevErroredSecs,
--        imaLinkTotalFeSevErroredSecs,
--        imaLinkTotalNeUnavailSecs,
--        imaLinkTotalFeUnavailSecs,
--        imaLinkTotalNeTxUnusableSecs,
--        imaLinkTotalNeRxUnusableSecs,
--        imaLinkTotalFeTxUnusableSecs,
--        imaLinkTotalFeRxUnusableSecs,
--        imaLinkTotalNeTxNumFailures,
--        imaLinkTotalNeRxNumFailures,
--        imaLinkTotalFeTxNumFailures,
--        imaLinkTotalFeRxNumFailures,
--        imaLinkTotalTxStuffs,
--        imaLinkTotalRxStuffs }
--      STATUS     mandatory
--      DESCRIPTION
--        "Objects containing interval statistics for an IMA link."
--      ::= { atmfImaMibGroups 7 }

--  imaNotificationsGroup NOTIFICATION-GROUP
--      NOTIFICATIONS {
--        imaFailureAlarm }
--      STATUS     mandatory
--      DESCRIPTION
--        "Notifications that must be implemented for IMA groups and links."
--      ::= { atmfImaMibGroups 8 }
END
