
		    Accton Technology Corporation
	     Ethernet Family LAN adapter board drivers


The drivers named "ACCNT" conform to the NDIS3 MiniPort Spec. It can support
Windows NT 3.5 and Windows 95 with different oemsetup.inf file.
This driver also support the Windows NT 3.1 but user must replace NDIS.SYS
by NT 3.5 DDK's NDIS.SYS (\DDK\SRC\NETWORK\NT31BIN\I386\FREE\NDIS.386)

File description:

	ACCNT.SYS    : NDIS3 MiniPort driver
	OEMSETUP.INF : Accton NT3.5 drivers information file
	NT35.TXT     : Read me file


컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴
Installing driver on Microsoft Windows NT3.5
컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴컴

   1)  In the Main group of NT, choose the Control Panel icon.

   2)  In the Control Panel window, choose the Network icon.

   3)  In the Network Settings dialog box, choose the Add Adapter button.
       The Add Network Adapter dialog box appears.

   4)  In the list of network cards, select "<other> Requires disk from
       manufacturer", and then press <Enter> button.

   5)  Insert this driver disk in drive A, enter drive and pathname A:\NT35
       and then choose the OK button.

   6)  In the Select OEM Option dialog box, you will see Accton EN166x MPX2
       PnP Adapter in the menu, use OK button to install it.

   7)  And then Accton EN166x MPX2 PnP Card Setup dialog box appear, you
       can specify "IRQ level" and "I/O Port Address" of the adapter plugged
       in your PC. However, this NDIS 3.0 mini port driver has support auto
       IO, IRQ scan for EN166x MPX2 adapter, so driver can work even user
       select a wrong IO port and IRQ.

       For multiple cards installation, specify correct IO port and IRQ is
       necessary.

   8)  After that, installation is completed. Accton's adapter becomes one
       of those Installed Adapter Cards and driver become one of those
       Installed Network Software. You can see: "[0x]Accton EN166x MPX2 PnP
       Adapter" within Installed Adapter Cards menu and "Accton EN166x MPX2
       PnP Adapter Driver" within Installed Network Software menu.

   9)  Now, the SYSTEM have already copied ACCNT.SYS from A:\NT35
       directory to C:\WINNT\SYSTEM32\DRIVERS and the OEMSETUP.INF form
       A:\NT35 to C:\WINNT\SYSTEM32 but renamed it to other installation
       information file. So next time, if you want to add Accton's adapters
       to your system, you do not need floppy diskette again.

  10)  To complete network installation, remember binding the adapter to
       transport drivers by choosing "Bindings" button under Network Setting
       dialog box.

  11)  Restarting your system you will acquire network service.


Trademarks:
Microsoft Windows NT is a trademark of Microsoft Corporation.


