950-1177-A 1

Intr oduction

The new Livingston Enterprises ComOS™ 3.3.3 softwar e release is now available for the PortMaster™ 2, 2E, 2ER, 2R and 25. This r elease is pr ovided at no char ge to all Livingston customers. The following document describes the featur es of the ComOS 3.3.3 softwar e release and how to upgrade your PortMaster . Upgrade instr uctions ar e included at the end of this r elease note.

WARNING! YOU MUST USE PMINST ALL VERSION 3.3.1 OR LA TER TO PERFORM THIS UPGRADE! If you ar e upgrading using PMconsole™ for W indows, you must use PMconsole for W indows version 1.1 or later . See “Upgrade Instr uctions” on page 2. If you have any port speeds set to 1 15200, upgrade to ComOS r elease 3.3.3, and later downgrade to any earlier r elease you must set the port speeds after downgrading.

New Featur e in ComOS 3.3.3

ComOS 3.3.3 includes the following new featur e:

For compatibility with the RADIUS RFC, Framed-Route attributes deliver ed from the RADIUS server which contain network masks of the type “/xx” no longer cr eate an error condition. The PortMaster strips the mask value fr om the destination addr ess and ignor es it.

Bug Fixes in ComOS 3.3.3

Basic rate ISDN lines using switch type 5ESS point-to-point (5ESS-PTP) now establish LAPD sessions on their D channels immediately after system startup. This allows some hunt gr oup pr ovisioning to work pr operly .

ISDN ports configur ed for “host pr ompt” now accept synchr onous PPP connections.

When dialing fr om one PortMaster to another using the V .120 protocol, users occasionally would not r eceive a login pr ompt until they pr essed the Enter key . This problem has been fixed.

ISDN calls made using Fr ench switch type VN4 now pass their called telephone number using the “unnumber ed” plan. This incr eases compatibility with some switches.

Calls r ejected due to service incompatibility now pr ovide pr oper cause codes to the switch.

A larger number of pr ocesses ar e now supported on the PM-2. This is r equir ed at boot time on a fully loaded PM-2E with 15 ISDN BRI ports.

The PortMaster occasionally r ebooted while auto-detecting asynchr onous PPP sessions. This pr oblem has been fixed.

ComOS 3.3.3 Release Note

ComOS 3.3.3 Release Note

2 ComOS 3.3.3

If a RADIUS server sent an Access-Challenge to users being authenticated with P AP the PortMaster incorr ectly tr eated it as an ACK. This has been fixed. An Access-Challenge r eceived for a P AP user is now tr eated as a NAK.

Memory Requir ements

If you ar e installing a MOD-10I-U or MOD-10I-ST expansion car d into a PM-2E-20 you should first install four megabytes of memory . This is the only har dwar e configuration that r equir es additional memory in ComOS 3.3.2 or 3.3.3. For instr uctions on upgrading the memory see the Communications Server Hardwar e Installation Guide.

Upgrade Instructions

If you ar e upgrading fr om ComOS 2.3 or 2.4 to 3.3.3, you must first upgrade to ComOS 3.0.4, reboot, then upgrade to 3.3.3.

If you have any port speeds set to 1 15200, upgrade to ComOS r elease 3.3.3. and downgrade to any r elease befor e 3.3.2 you must set the port speeds again after downgrading.

WARNING! YOU MUST USE PMINST ALL VERSION 3.3.1 OR LA TER TO PERFORM THIS UPGRADE! If you ar e upgrading using PMconsole™ for W indows, you must use PMconsole for W indows version 1.1 or later .

The 3.3.3 upgrade image is available for the PortMaster 2, 2E, 2ER, and 2R at

ftp://ftp.livingston.com/pub/le/upgrades/pm2_3.3.3 and for the

PortMaster 25 at ftp://ftp.livingston.com/pub/le/upgrades/pm25_3.3.3.

ComOS 3.3.3 uses the same RADIUS dictionary file as ComOS 3.3.2. The dictionary file is available at ftp://ftp.livingston.com/pub/le/radius/dictionary.

The installation softwar e can be FTPed fr om

ftp://ftp.livingston.com/pub/le/software/system/tarfile.

To upgrade a PM-2, PM-2E, PM-2ER, or PM-2R to ComOS 3.3.3, r un pminstall and choose the Upgrade PortMaster option, choose pm2_3.3.3 from the menu of upgrade choices, enter your PortMaster ’s hostname or IP addr ess, and enter your PortMaster ’s administrative passwor d. pminstall upgrades your PortMaster to ComOS 3.3.3.

To upgrade a PM-25 follow the above instr uctions except choose pm25_3.3.3 from the menu of upgrade choices instead of pm2_3.3.3.

The upgrade does not af fect your stor ed configuration in the PortMaster . If you would like to backup your PortMaster configuration befor e upgrading, r un pmreadconf:

umask 22
mkdir /usr/portmaster
cd /usr/portmaster
tar xvf tarfile
./pminstall

cd /usr/portmaster
./pmreadconf pmname pmpassword data/pmname.conf
chmod 600 data/pmname.conf

ComOS 3.3.3 Release Note

Copyright and Trademarks 3

Copyright and T rademarks

© 1996 Livingston Enterprises, Inc. All rights r eserved.

The pr oduct names, “ComOS,” “IRX,” “PortMaster ,” “PMconsole,” and “T elePath” ar e trademarks belonging to Livingston Enterprises, Inc.

All brand pr oduct names mentioned in this document ar e trademarks or r egister ed trademarks of their r espective manufactur ers.

Notices

Livingston Enterprises, Inc. makes no r epresentations or warranties with r espect to the contents or use of this manual, and specifically disclaims any expr ess or implied warranties of mer chantability or fitness for any particular purpose. Further , Livingston Enterprises, Inc. r eserves the right to r evise this publication and to make changes to its content, any time, without obligation to notify any person or entity of such r evisions or changes.

Contacting Livingston T echnical Support

Every Livingston PortMaster or IRX™ pr oduct comes with fr ee lifetime softwar e technical support and a one year hardwar e warranty . Livingston Enterprises pr ovides fr ee technical support via voice, F AX, and electr onic mail. Technical support is available Monday thr ough Friday 6am-5pm Pacific T ime (GMT-8).

To contact Livingston technical support by voice, dial 1-800-458-9966 within the US or 1-510-426-0770 outside the US, by F AX, dial 1-510-426-8951, by electr onic mail, send mail to support@livingston.com, and thr ough the W orld W ide Web at http://www .livingston.com/.